,Capacity Cooling (HP)##other##,Compressor Motor Output (W)##other##,Compressor Type##other##,Drain Outlet Diameter1##other##,Cooling Capacity (kcal/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(mm)##other##,Free Contents Download##other##,Heat Exchanger Head Loss (kPa)##other##,Heat Exchanger Maximum Pressure Resistance (kg/cm2)##other##,Heat Exchanger Rated Water Flow (LPM)##other##,Heat Exchanger Type##other##,Heating Capacity (kcal/h)##other##,Heating Capacity (kW)##other##,Independent Unit##other##,Indoor Unit Model Max Quantity##other##,Indoor Unit Total Capacity##other##,MCA (A)##other##,Model name##other##,Net Weight (kg)##other##,Pipe Connection_Common Side (mm)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,"Power Supply (Ph,V,Hz)"##other##,Refrigerant Charge (Kg)##other##,Gas Pipe Diameter1##other##,Liquid Pipe Diameter1##other##,Refrigerant Type##other##,Sound Pressure Level Cooling/Heating (dB(A))##other##,Temp Operating Range (Cooling)(C)##other##,Temp Operating Range (Heating)(C)##other##,Transmission Cable##other##,Type##other##,Water Inlet Pipe Diameter1##other##,Water Outlet Pipe Diameter1##other##
"ARWN80LAS4",8,4200, Hermetically Sealed Scroll  ,20,19300,22.4,(755 x 500 x 997) x 1,http://www.lgeaircon.com/,36.5,45,77,Stainless Steel Plate,21700,25.2,ARWN80LAS4,20,50% to 130% of Outdoor Unit Capacity,24,ARWN80LAS4,120 x 1,19.05,20,3/4,19.05,3/8,9.52,3.86,4.2,"380-415,3,50/380,3,60",5.5,19.05,9.52,R410A,47/51,10 ~ 45,-5 ~ 45,1.0 ~1.5 x 2C,Multi V Water lV,32,32
"ARWN100LAS4",10,4200, Hermetically Sealed Scroll  ,20,24100,28,(755 x 500 x 997) x 1,http://www.lgeaircon.com/,36.5,45,96,Stainless Steel Plate,27100,31.5,ARWN100LAS4,25,50% to 130% of Outdoor Unit Capacity,24.5,ARWN100LAS4,120 x 1,19.05,20,7/8,22.2,3/8,9.52,5.09,5.34,"380-415,3,50/380,3,60",3.4,22.2,9.52,R410A,50/53,10 ~ 45,-5 ~ 45,1.0 ~1.5 x 2C,Multi V Water lV,32,32
"ARWN120LAS4",12,4200, Hermetically Sealed Scroll  ,20,28900,33.6,(755 x 500 x 997) x 1,http://www.lgeaircon.com/,36.5,45,116,Stainless Steel Plate,32500,37.8,ARWN120LAS4,30,50% to 130% of Outdoor Unit Capacity,25,ARWN120LAS4,120 x 1,19.05,20,1,25.4,1/2,12.7,6.46,6.75,"380-415,3,50/380,3,60",3.5,25.4,12.7,R410A,56/56,10 ~ 45,-5 ~ 45,1.0 ~1.5 x 2C,Multi V Water lV,32,32
"ARWN140LAS4",14,4200, Hermetically Sealed Scroll  ,20,33700,39.2,(755 x 500 x 997) x 1,http://www.lgeaircon.com/,36.5,45,135,Stainless Steel Plate,37900,44.1,ARWN140LAS4,35,50% to 130% of Outdoor Unit Capacity,25.5,ARWN140LAS4,120 x 1,19.05,20,1,25.4,1/2,12.7,7.84,8.17,"380-415,3,50/380,3,60",5.8,25.4,12.7,R410A,58/57,10 ~ 45,-5 ~ 45,1.0 ~1.5 x 2C,Multi V Water lV,40,40
"ARWN160LAS4",16,5300, Hermetically Sealed Scroll  ,20,38500,44.8,(755 x 500 x 997) x 1,http://www.lgeaircon.com/,31.8,45,154,Stainless Steel Plate,43300,50.4,ARWN160LAS4,40,50% to 130% of Outdoor Unit Capacity,32,ARWN160LAS4,140 x 1,19.05,20,1-1/8,28.58,1/2,12.7,8.15,8.54,"380-415,3,50/380,3,60",5.8,28.58,12.7,R410A,53/57,10 ~ 45,-5 ~ 45,1.0 ~1.5 x 2C,Multi V Water lV,40,40
"ARWN180LAS4",18,5300, Hermetically Sealed Scroll  ,20,43300,50.4,(755 x 500 x 997) x 1,http://www.lgeaircon.com/,31.8,45,173,Stainless Steel Plate,48800,56.7,ARWN180LAS4,45,50% to 130% of Outdoor Unit Capacity,32.5,ARWN180LAS4,140 x 1,19.05,20,1-1/8,28.58,1/2,12.7,9.69,10.13,"380-415,3,50/380,3,60",3.5,28.58,12.7,R410A,55/56,10 ~ 45,-5 ~ 45,1.0 ~1.5 x 2C,Multi V Water lV,40,40
"ARWN200LAS4",20,5300,Hermetically Sealed Scroll,20,48200,56,(755 x 500 x 997) x 1,http://www.lgeaircon.com/,31.8,45,192,Stainless Steel Plate,54200,63,ARWN200LAS4,44,50% to 130% of Outdoor Unit Capacity,33,ARWN200LAS4,140 x 1,19.05,20,1-1/8,28.58,1/2,12.7,11.2,11.67,"380-415,3,50/380,3,60",3.4,28.58,12.7,R410A,54/60,10 ~ 45,-5 ~ 45,1.0 ~1.5 x 2C,Multi V Water lV,40,40

