,Casing##other##,Chassis name##other##,Communication Cable (mm2)##other##,Compressor Motor Output (W)##other##,Compressor Type##other##,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxDxH)(inch)##other##,Dimensions (WxDxH)(mm)##other##,Free Contents Download##other##,Heat Exchanger Head Loss (kPa/ft.wg)##other##,Heat Exchanger Rated Water Flow (lpm/GPM)##other##,Heat Exchanger Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,MCA (A)##other##,Model name##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Power Input (Heating/Cooling)(kW)##other##,Power Input (Heating/Cooling)(W)##other##,"Power Supply (Ph,V,Hz)"##other##,Refrigerant Charge (Kg)##other##,Refrigerant Charge (lbs)##other##,Refrigerant Gas Connection Diameter(mm)##other##,Refrigerant Gas Connection Radius(mm)##other##,Refrigerant Liquid Connection Diameter(mm)##other##,Refrigerant Liquid Connection Radius(mm)##other##,Refrigerant Type##other##,Sound Pressure Level Cooling (dB(A))##other##,Sound Pressure Level Heating (dB(A))##other##,Water Inlet Connection Diameter(mm)##other##,Water Inlet Connection Radius(mm)##other##,Water Outlet Connection Diameter(mm)##other##,Water Outlet Connection Radius(mm)##other##
"ARWN40GA0",Warm Gray,K3,2C X 1.0 ~ 1.5,4000,BLDC Inverter Twin Rotary,"38,200",11.2,20-1/2 x 42-1/2 x 13,"520 x 1,080 x 330",http://www.lgeaircon.com/,(14.0/4.7),(40 /10.6),Cupro brazed Stainless Steel Plate,"42,600",12.5,26,ARWN40GA0,76,168,2.10,2.20,"220-240,1,50 / 220,1,60",1,2.2,19.05,9.525,9.52,4.76,R410A,47,48,32,16,32,16
"ARWN50GA0",Warm Gray,K3,2C X 1.0 ~ 1.5,"4,000",BLDC Inverter Twin Rotary,"47,800",14.0,20-1/2 x 42-1/2 x 13,"520 x 1,080 x 330",http://www.lgeaircon.com/,(20.7/6.9),(50 /13.2),Cupro brazed Stainless Steel Plate,"54,600",16.0,26,ARWN50GA0,76,168,2.70,2.90,"220-240,1,50 / 220,1,60",1,2.2,19.05,9.525,9.52,4.76,R410A,48,49,32,16,32,16
"ARWN60GA0",Warm Gray,K3,2C X 1.0 ~ 1.5,"4,000",BLDC Inverter Twin Rotary,"52,900",15.5,20-1/2 x 42-1/2 x 13,"520 x 1,080 x 330",http://www.lgeaircon.com/,(28.4/9.5),(60 /15.9),Cupro brazed Stainless Steel Plate,"61,400",18.0,26,ARWN60GA0,76,168,3.20,3.50,"220-240,1,50 / 220,1,60",1,2.2,19.05,9.525,9.52,4.76,R410A,49,50,32,16,32,16

