,Product Type##other##,Model Name_Buyer##other##,Model Name_Factory##other##,Chassis Name##other##,Dimensions (W x D x H) (mm)##other##,Dimensions (W x D x H) (inch)##other##,Drain Hose Diameter_Inner (mm)##other##,Drain Hose Diameter_Inner (inch)##other##,Drain Hose Diameter_Outer (mm)##other##,Drain Hose Diameter_Outer (inch)##other##,Piping Diameter_Gas (mm)##other##,Piping Diameter_Gas (inch)##other##,Piping Diameter_Liquid (mm)##other##,Piping Diameter_Liquid (inch)##other##,Power Supply (Ph_V_Hz)##other##,Power and Communication Cable (No x mm2)##other##,Power and Communication Cable (No x AWG)##other##,Running Current_Rated_Cooling (A)##other##,Running Current_Rated_Heating (A)##other##,Air Flow Rate_Cooling (Max / H / M / L) (CMM)##other##,Air Flow Rate_Cooling (Max / H / M / L) (CFM)##other##,Air Flow Rate_Heating (Max / H / M / L) (CMM)##other##,Air Flow Rate_Heating (Max / H / M / L) (CFM)##other##,Capacity_Rated_Cooling (kW)##other##,Capacity_Rated_Cooling (Btu/h)##other##,Capacity_Rated_Heating (kW)##other##,Capacity_Rated_Heating (Btu/h)##other##,Power Input_Rated_Cooling (W)##other##,Power Input_Rated_Heatling (W)##other##,Exterior Color Code##other##,Fan Type##other##,Fan Motor Output (W)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Refrigerant Type##other##,Sound Pressure Level_Cooling (Max / H / M / L / SL) (dB(A))##other##,Sound Pressure Level_Heating (Max / H / M / L) (dB(A))##other##
"P24EN.NSK",Wall Mounted,P24EN.NSK,USNW246K3A0,SK,998 x 345 x 210,-,16.0,5/8,21.5,27/32,15.88,5/8,6.35,1/4,1_220-240_50,4 x 1.0,-,10.10,10.40,20.0 / 16.1 / 13.1 / 10.5,20.5 / 18.5 / 15.0 / 11.0,-,-,6.60,22520,7.50,25591,2275,2308,Munsell 7.5BG 10/2 (RAL 9016),Cross Flow Fan,60,12.5,27.6,R410A,50 / 47 / 42 / 34 / 31,50 / 47 / 42 / 34
"DM24RP.NSK",Wall Mounted,DM24RP.NSK,ASNW24GK1Z0,SK,998 x 345 x 210,-,16.0,5/8,21.5,27/32,15.88,5/8,6.35,1/4,1_220-240_50,4 x 1.0,-,10.10,10.40,20.0 / 16.1 / 13.1 / 10.5,20.5 / 18.5 / 15.0 / 11.0,-,-,6.60,22520,7.50,25591,2275,2238,Munsell 7.5BG 10/2 (RAL 9016),Cross Flow Fan,60,12.0,26.5,R410A,50 / 47 / 42 / 34 / 31,50 / 47 / 42 / 34
"PM24SP.NSK",Wall Mounted,PM24SP.NSK,USNW24GK2F0,SK,998 x 345 x 210,-,16.0,5/8,21.5,27/32,15.88,5/8,6.35,1/4,1_220-240_50,4 x 1.0,-,10.10,10.40,20.0 / 16.1 / 13.1 / 10.5,20.5 / 18.5 / 15.0 / 11.0,-,-,6.60,22520,7.50,25591,2275,2308,Munsell 7.5BG 10/2 (RAL 9016),Cross Flow Fan,60,12.8,28.2,R410A,50 / 47 / 42 / 34 / 31,50 / 47 / 42 / 34

