,Product Type##other##,Model Name_Buyer##other##,Model Name_Factory##other##,Chassis Name##other##,Dimensions (W x D x H) (mm)##other##,Dimensions (W x D x H) (inch)##other##,Piping Diameter_Gas (mm)##other##,Piping Diameter_Gas (inch)##other##,Piping Diameter_Liquid (mm)##other##,Piping Diameter_Liquid (inch)##other##,Maximum Overcurrent Protection (MOP) (A)##other##,Power Supply (Ph_V_Hz)##other##,Power Supply Cable (No x mm2)##other##,Power Supply Cable (No x AWG)##other##,Power and Communication Cable (No x mm2)##other##,Power and Communication Cable (No x AWG)##other##,Running Current_Rated_Cooling (A)##other##,Running Current_Rated_Heating (A)##other##,Air Flow Rate_Max (CMM)##other##,Air Flow Rate_Max (CFM)##other##,Capacity_Rated_Cooling (kW)##other##,Capacity_Rated_Cooling (Btu/h)##other##,Capacity_Rated_Heating (kW)##other##,Capacity_Rated_Heating (Btu/h)##other##,Power Input_Rated_Cooling (W)##other##,Power Input_Rated_Heatling (W)##other##,Compressor Type##other##,Exterior Color Code##other##,Fan Type##other##,Fan Motor Type##other##,Fan Motor Output (W)##other##,Max Elevation Difference (m)##other##,Max Elevation Difference (ft)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Operation Range Temperature_Cooling (C)##other##,Operation Range Temperature_Cooling (F)##other##,Operation Range Temperature_Heating (C)##other##,Operation Range Temperature_Heating (F)##other##,Piping Length_Min / Standard / Max (m)##other##,Piping Length_Min / Standard / Max (ft)##other##,Piping Length_No Charge (m)##other##,Piping Length_No Charge (ft)##other##,Refrigerant Type##other##,Refrigerant_Precharge (g)##other##,Refrigerant_Precharge (oz)##other##,Refrigerant_Additional Charge (g/m)##other##,Refrigerant_Additional Charge (oz/ft)##other##,Sound Pressure Level_Rated_Cooling (dB(A))##other##,Sound Pressure Level_Rated_Heating (dB(A))##other##
"P18EN.UL2",Single Inverter,P18EN.UL2,USUW186K3A0,UL2,770 x 545 x 288,-,12.7,1/2,6.35,1/4,20,1_220-240_50,3 x 1.5,-,4 x 1.0,-,6.90,7.10,35.0,-,5.00,17072,5.80,19804,1587,1611,Twin Rotary,Munsell 9.54Y 8.34/1.31 (RAL 9001),Propeller Fan,BLDC,43,10,32.8,36.7,80.9,-15 ~ 48,-,-10 ~ 18,-,3 / 7.5 / 20,9.8 / 24.6 / 65.6,7.5,24.6,R410A,1200,42.3,20,0.22,53,55
"DM18RP.UL2",Single Inverter,DM18RP.UL2,ASUW18GK1Z0,UL2,770 x 545 x 288,-,12.7,1/2,6.35,1/4,20,1_220-240_50,3 x 1.5,-,4 x 1.0,-,6.90,7.10,35.0,-,5.00,17060,5.80,19790,1562,1611,Twin Rotary,Munsell 9.54Y 8.34/1.31 (RAL 9001),Propeller Fan,BLDC,43,10,32.8,36.2,79.8,-15 ~ 48,-,-10 ~ 18,-,3 / 7.5 / 20,9.8 / 24.6 / 65.6,7.5,24.6,R410A,1250,44.1,20,0.22,53,55
"PM18SP.UL2",Single Inverter,PM18SP.UL2,USUW18GK2F0,UL2,770 x 545 x 288,-,12.7,1/2,6.35,1/4,20,1_220-240_50,3 x 1.5,-,4 x 1.0,-,6.90,7.10,35.0,-,5.00,17072,5.80,19804,1587,1611,Twin Rotary,Munsell 9.54Y 8.34/1.31 (RAL 9001),Propeller Fan,BLDC,43,10,32.8,36.3,80,-15 ~ 48,-,-10 ~ 18,-,3 / 7.5 / 20,9.8 / 24.6 / 65.6,7.5,24.6,R410A,1200,42.3,20,0.22,53,55
"PM18EP.UL2",Single Inverter,PM18EP.UL2,USUW18GK3A0,UL2,770 x 545 x 288,-,12.7,1/2,6.35,1/4,20,1_220-240_50,3 x 1.5,-,4 x 1.0,-,6.90,7.10,35.0,-,5.00,17072,5.80,19804,1587,1611,Twin Rotary,Munsell 9.54Y 8.34/1.31 (RAL 9001),Propeller Fan,BLDC,43,10,32.8,36.7,80.9,-15 ~ 48,-,-10 ~ 18,-,3 / 7.5 / 20,9.8 / 24.6 / 65.6,7.5,24.6,R410A,1200,42.3,20,0.22,53,55
"AM18BP.UL2",Single Inverter,AM18BP.UL2,USUW18GKRZ0,UL2,770 x 545 x 288,-,12.7,1/2,6.35,1/4,20,1_220-240_50,3 x 1.5,-,4 x 1.0,-,6.90,7.10,35.0,-,5.00,17072,5.80,19804,1587,1611,Twin Rotary,Munsell 9.54Y 8.34/1.31 (RAL 9001),Propeller Fan,BLDC,43,10,32.8,36.3,80,-15 ~ 48,-,-10 ~ 18,-,3 / 7.5 / 20,9.8 / 24.6 / 65.6,7.5,24.6,R410A,1200,42.3,20,0.22,53,55

