,Manufacturer##other##,Model Name (Buyer)##other##,Model Name (Factory)##other##,Type##other##,Chassis Name##other##,Free Contents Download##other##,Color##other##,Cooling Capacity (kW)##other##,Heating Capacity (kW)##other##,Power Input (Cooling) (W)##other##,Power Input (Heatling) (W)##other##,Running Current (Cooling) (A)##other##,Running Current (Heating) (A)##other##,"Power Supply (Ph, V, Hz)"##other##,Air Flow Rate (Cooling) (Max / H / M / L) (CMM)##other##,Air Flow Rate (Heating) (Max / H / M / L) (CMM)##other##,Sound Pressure Level (Cooling) (H / M / L / SL) (dB(A))##other##,Sound Pressure Level (Heating) (H / M / L) (dB(A))##other##,Fan Type##other##,Fan Motor Output (W)##other##,Power and Communication Cable (No x mm2)##other##,Refrigerant Liquid Connection Diameter (mm)##other##,Refrigerant Gas Connection Diameter (mm)##other##,Condensate Drain Connection Outside Diameter (mm)##other##,Condensate Drain Connection Inside Diameter (mm)##other##,Width (mm)##other##,Height (mm)##other##,Depth (mm)##other##,Net Weight (kg)##other##,Refrigerant Type##other##
"G09WL.NS3",LG,G09WL.NS3,ASNW0963WB0,Wall Mounted,S3,http://www.lgeaircon.com/,White,2.50,3.00,690,830,4.00,4.00,"1, 220-240, 50",9.7 / - / - / -,- / - / - / -,39 / 34 / 29 / -,39 / 35 / 32,Turbo Fan,32.7,4C x 1.0,6.35,9.52,21.5,16.0,645,645,121,18.0,R410A
"G12WL.NS3",LG,G12WL.NS3,ASNW1263WB0,Wall Mounted,S3,http://www.lgeaircon.com/,White,3.50,3.50,1090,970,5.00,4.50,"1, 220-240, 50",10.5 / - / - / -,- / - / - / -,39 / 34 / 29 / -,39 / 35 / 32,Turbo Fan,32.7,4C x 1.0,6.35,9.52,21.5,16.0,645,645,121,18.0,R410A

