,Product Type##other##,Model Name_Buyer##other##,Model Name_Factory##other##,Chassis Name##other##,Dimensions (W x D x H) (mm)##other##,Dimensions (W x D x H) (inch)##other##,Drain Hose Diameter_Inner (mm)##other##,Drain Hose Diameter_Inner (inch)##other##,Drain Hose Diameter_Outer (mm)##other##,Drain Hose Diameter_Outer (inch)##other##,Piping Diameter_Gas (mm)##other##,Piping Diameter_Gas (inch)##other##,Piping Diameter_Liquid (mm)##other##,Piping Diameter_Liquid (inch)##other##,Power Supply (Ph_V_Hz)##other##,Power and Communication Cable (No x mm2)##other##,Power and Communication Cable (No x AWG)##other##,Running Current_Rated_Cooling (A)##other##,Running Current_Rated_Heating (A)##other##,Air Flow Rate_Cooling (Max / H / M / L) (CMM)##other##,Air Flow Rate_Cooling (Max / H / M / L) (CFM)##other##,Air Flow Rate_Heating (Max / H / M / L) (CMM)##other##,Air Flow Rate_Heating (Max / H / M / L) (CFM)##other##,Capacity_Rated_Cooling (kW)##other##,Capacity_Rated_Cooling (Btu/h)##other##,Capacity_Rated_Heating (kW)##other##,Capacity_Rated_Heating (Btu/h)##other##,Power Input_Rated_Cooling (W)##other##,Power Input_Rated_Heatling (W)##other##,Exterior Color Code##other##,Fan Type##other##,Fan Motor Output (W)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Refrigerant Type##other##,Sound Pressure Level_Cooling (Max / H / M / L / SL) (dB(A))##other##,Sound Pressure Level_Heating (Max / H / M / L) (dB(A))##other##
"AM09BP.NSJ",Wall Mounted,AM09BP.NSJ,USNW09GJRZ0,SJ,837 x 308 x 192,-,16.0,5/8,21.5,27/32,9.52,3/8,6.35,1/4,1_220-240_50,4 x 1.0,-,3.00,3.70,11.5 / 10.0 / 7.5 / 4.2,12.0 / 10.0 / 7.2 / 5.6,-,-,2.50,8531,3.20,10919,670,840,Munsell 7.5PB 0.2/20 (RAL 9005),Cross Flow Fan,30,9.9,21.8,R410A,44 / 41 / 35 / 27 / 19,44 / 41 / 35 / 27
"AM12BP.NSJ",Wall Mounted,AM12BP.NSJ,USNW12GJRZ0,SJ,837 x 308 x 192,-,16.0,5/8,21.5,27/32,9.52,3/8,6.35,1/4,1_220-240_50,4 x 1.0,-,4.70,4.50,12.5 / 10.0 / 7.5 / 4.2,13.0 / 10.0 / 7.2 / 5.6,-,-,3.50,12000,3.80,13000,1080,1000,Munsell 7.5PB 0.2/20 (RAL 9005),Cross Flow Fan,30,9.9,21.8,R410A,45 / 41 / 35 / 27 / 19,45 / 41 / 35 / 27

