,Product Type##other##,Model Name_Buyer##other##,Model Name_Factory##other##,Chassis Name##other##,Dimensions (W x D x H) (mm)##other##,Dimensions (W x D x H) (inch)##other##,Piping Diameter_Gas (mm)##other##,Piping Diameter_Gas (inch)##other##,Piping Diameter_Liquid (mm)##other##,Piping Diameter_Liquid (inch)##other##,Maximum Overcurrent Protection (MOP) (A)##other##,Power Supply (Ph_V_Hz)##other##,Power Supply Cable (No x mm2)##other##,Power Supply Cable (No x AWG)##other##,Power and Communication Cable (No x mm2)##other##,Power and Communication Cable (No x AWG)##other##,Running Current_Rated_Cooling (A)##other##,Running Current_Rated_Heating (A)##other##,Air Flow Rate_Max (CMM)##other##,Air Flow Rate_Max (CFM)##other##,Capacity_Rated_Cooling (kW)##other##,Capacity_Rated_Cooling (Btu/h)##other##,Capacity_Rated_Heating (kW)##other##,Capacity_Rated_Heating (Btu/h)##other##,Power Input_Rated_Cooling (W)##other##,Power Input_Rated_Heatling (W)##other##,Compressor Type##other##,Exterior Color Code##other##,Fan Type##other##,Fan Motor Type##other##,Fan Motor Output (W)##other##,Max Elevation Difference (m)##other##,Max Elevation Difference (ft)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Operation Range Temperature_Cooling (C)##other##,Operation Range Temperature_Cooling (F)##other##,Operation Range Temperature_Heating (C)##other##,Operation Range Temperature_Heating (F)##other##,Piping Length_Min / Standard / Max (m)##other##,Piping Length_Min / Standard / Max (ft)##other##,Piping Length_No Charge (m)##other##,Piping Length_No Charge (ft)##other##,Refrigerant Type##other##,Refrigerant_Precharge (g)##other##,Refrigerant_Precharge (oz)##other##,Refrigerant_Additional Charge (g/m)##other##,Refrigerant_Additional Charge (oz/ft)##other##,Sound Pressure Level_Rated_Cooling (dB(A))##other##,Sound Pressure Level_Rated_Heating (dB(A))##other##
"DC09RQ.UL2",Single Inverter,DC09RQ.UL2,S3UM09JL1ZA,UL2,770 x 545 x 288,-,9.52,3/8,6.35,1/4,15,1_220-240_50,3 x 1,-,4 x 1,-,2.50,3.20,35.0,-,2.50,8536,3.20,10926,572,711,Twin Rotary,Munsell 9.54Y 8.34/1.31 (RAL 9001),Propeller Fan,BLDC,43,10,32.8,34.1,75.2,-15 ~ 48 (DB),-,-15 ~ 18 (WB),-,3 / 7.5 / 20,9.8 / 24.6 / 65.6,12.5,41.0,R32,800,28.2,20,0.22,49,51
"DC12RQ.UL2",Single Inverter,DC12RQ.UL2,S3UM12JL1ZA,UL2,770 x 545 x 288,-,9.52,3/8,6.35,1/4,15,1_220-240_50,3 x 1,-,4 x 1,-,4.00,4.30,35.0,-,3.50,11950,4.00,13658,933,976,Twin Rotary,Munsell 9.54Y 8.34/1.31 (RAL 9001),Propeller Fan,BLDC,43,10,32.8,34.1,75.2,-15 ~ 48 (DB),-,-15 ~ 18 (WB),-,3 / 7.5 / 20,9.8 / 24.6 / 65.6,12.5,41.0,R32,800,28.2,20,0.22,49,51

