,Product Type##other##,Model Name_Buyer##other##,Model Name_Factory##other##,Chassis Name##other##,Dimensions (W x D x H) (mm)##other##,Dimensions (W x D x H) (inch)##other##,Drain Hose Diameter_Inner (mm)##other##,Drain Hose Diameter_Inner (inch)##other##,Drain Hose Diameter_Outer (mm)##other##,Drain Hose Diameter_Outer (inch)##other##,Piping Diameter_Gas (mm)##other##,Piping Diameter_Gas (inch)##other##,Piping Diameter_Liquid (mm)##other##,Piping Diameter_Liquid (inch)##other##,Power Supply (Ph_V_Hz)##other##,Power and Communication Cable (No x mm2)##other##,Power and Communication Cable (No x AWG)##other##,Running Current_Rated_Cooling (A)##other##,Running Current_Rated_Heating (A)##other##,Air Flow Rate_Cooling (Max / H / M / L) (CMM)##other##,Air Flow Rate_Cooling (Max / H / M / L) (CFM)##other##,Air Flow Rate_Heating (Max / H / M / L) (CMM)##other##,Air Flow Rate_Heating (Max / H / M / L) (CFM)##other##,Capacity_Rated_Cooling (kW)##other##,Capacity_Rated_Cooling (Btu/h)##other##,Capacity_Rated_Heating (kW)##other##,Capacity_Rated_Heating (Btu/h)##other##,Power Input_Rated_Cooling (W)##other##,Power Input_Rated_Heatling (W)##other##,Exterior Color Code##other##,Fan Type##other##,Fan Motor Output (W)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Refrigerant Type##other##,Sound Pressure Level_Cooling (Max / H / M / L / SL) (dB(A))##other##,Sound Pressure Level_Heating (Max / H / M / L) (dB(A))##other##
"S09ER.NSW",Wall Mounted,S09ER.NSW,S3NW09WA5AA,SW+,756 x 265 x 184,-,16.0,5/8,21.5,27/32,9.52,3/8,6.35,1/4,1_220-240_50,4 x 1,-,3.50,4.40,7.5 / 6 / 4.5 / 3.8,-,9 / 7 / 6 / 5,-,2.50,8530,3.20,10918,731,950,Munsell 7.5BG 10/2 (RAL 9016),Cross Flow Fan,30,7.5,16.5,R32,- / 42 / 36 / 28 / 22,- / 42 / 36 / 28

