,Product Type##other##,Model Name_Buyer##other##,Model Name_Factory##other##,Chassis Name##other##,Dimensions (W x D x H) (mm)##other##,Dimensions (W x D x H) (inch)##other##,Piping Diameter_Gas (mm)##other##,Piping Diameter_Gas (inch)##other##,Piping Diameter_Liquid (mm)##other##,Piping Diameter_Liquid (inch)##other##,Maximum Overcurrent Protection (MOP) (A)##other##,Power Supply (Ph_V_Hz)##other##,Power Supply Cable (No x mm2)##other##,Power Supply Cable (No x AWG)##other##,Power and Communication Cable (No x mm2)##other##,Power and Communication Cable (No x AWG)##other##,Running Current_Rated_Cooling (A)##other##,Running Current_Rated_Heating (A)##other##,Air Flow Rate_Max (CMM)##other##,Air Flow Rate_Max (CFM)##other##,Capacity_Rated_Cooling (kW)##other##,Capacity_Rated_Cooling (Btu/h)##other##,Capacity_Rated_Heating (kW)##other##,Capacity_Rated_Heating (Btu/h)##other##,Power Input_Rated_Cooling (W)##other##,Power Input_Rated_Heatling (W)##other##,Compressor Type##other##,Exterior Color Code##other##,Fan Type##other##,Fan Motor Type##other##,Fan Motor Output (W)##other##,Max Elevation Difference (m)##other##,Max Elevation Difference (ft)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Operation Range Temperature_Cooling (C)##other##,Operation Range Temperature_Cooling (F)##other##,Operation Range Temperature_Heating (C)##other##,Operation Range Temperature_Heating (F)##other##,Piping Length_Min / Standard / Max (m)##other##,Piping Length_Min / Standard / Max (ft)##other##,Piping Length_No Charge (m)##other##,Piping Length_No Charge (ft)##other##,Refrigerant Type##other##,Refrigerant_Precharge (g)##other##,Refrigerant_Precharge (oz)##other##,Refrigerant_Additional Charge (g/m)##other##,Refrigerant_Additional Charge (oz/ft)##other##,Sound Pressure Level_Rated_Cooling (dB(A))##other##,Sound Pressure Level_Rated_Heating (dB(A))##other##
"DC18RQ.UL2",Single Inverter,DC18RQ.UL2,S3UM18KL1ZA,UL2,770 x 545 x 288,-,12.7,1/2,6.35,1/4,20,1_220-240_50,3 x 1.5,-,4 x 1,-,6.90,7.10,35.0,-,5.00,17072,5.80,19804,1562,1611,Twin Rotary,Munsell 9.54Y 8.34/1.31 (RAL 9001),Propeller Fan,BLDC,43,10,32.8,34.4,75.8,-15 ~ 48 (DB),-,-10 ~ 18 (WB),-,3 / 7.5 / 20,9.8 / 24.6 / 65.6,7.5,24.6,R32,1000,35.3,20,0.22,53,55
"PC18SQ.UL2",Single Inverter,PC18SQ.UL2,S3UM18KL2FA,UL2,770 x 545 x 288,-,12.7,1/2,6.35,1/4,20,1_220-240_50,3 x 1.5,-,4 x 1,-,6.90,7.10,35.0,-,5.00,17072,5.80,19804,1562,1611,Twin Rotary,Munsell 9.54Y 8.34/1.31 (RAL 9001),Propeller Fan,BLDC,43,10,32.8,34.4,75.8,-15 ~ 48 (DB),-,-10 ~ 18 (WB),-,3 / 7.5 / 20,9.8 / 24.6 / 65.6,7.5,24.6,R32,1000,35.3,20,0.22,53,55
"S18EQ.UL2",Single Inverter,S18EQ.UL2,S3UW18KL3BA,UL2,770 x 545 x 288,-,12.7,1/2,6.35,1/4,20,1_220-240_50,3 x 1.5,-,4 x 1,-,6.90,7.10,35.0,-,5.00,17072,5.80,19804,1562,1611,Twin Rotary,Munsell 9.54Y 8.34/1.31 (RAL 9001),Propeller Fan,BLDC,43,10,32.8,34.4,75.8,-15 ~ 48 (DB),-,-10 ~ 18 (WB),-,3 / 7.5 / 20,9.8 / 24.6 / 65.6,7.5,24.6,R32,1000,35.3,20,0.22,53,55
"SC18EQ.UL2",Single Inverter,SC18EQ.UL2,S3UM18KL3BA,UL2,770 x 545 x 288,-,12.7,1/2,6.35,1/4,20,1_220-240_50,3 x 1.5,-,4 x 1,-,6.90,7.10,35.0,-,5.00,17072,5.80,19804,1562,1611,Twin Rotary,Munsell 9.54Y 8.34/1.31 (RAL 9001),Propeller Fan,BLDC,43,10,32.8,34.4,75.8,-15 ~ 48 (DB),-,-10 ~ 18 (WB),-,3 / 7.5 / 20,9.8 / 24.6 / 65.6,7.5,24.6,R32,1000,35.3,20,0.22,53,55
"AC18BQ.UL2",Single Inverter,AC18BQ.UL2,S3UM18KLRZA,UL2,770 x 545 x 288,-,12.7,1/2,6.35,1/4,20,1_220-240_50,3 x 1.5,-,4 x 1,-,6.90,7.10,35.0,-,5.00,17072,5.80,19804,1562,1611,Twin Rotary,Munsell 9.54Y 8.34/1.31 (RAL 9001),Propeller Fan,BLDC,43,10,32.8,35.2,77.6,-15 ~ 48 (DB),-,-10 ~ 18 (WB),-,3 / 7.5 / 20,9.8 / 24.6 / 65.6,7.5,24.6,R32,1000,35.3,20,0.22,53,55

