,Product Type##other##,Model Name_Buyer##other##,Model Name_Factory##other##,Chassis Name##other##,Dimensions (W x D x H) (mm)##other##,Dimensions (W x D x H) (inch)##other##,Piping Diameter_Gas (mm)##other##,Piping Diameter_Gas (inch)##other##,Piping Diameter_Liquid (mm)##other##,Piping Diameter_Liquid (inch)##other##,Maximum Overcurrent Protection (MOP) (A)##other##,Power Supply (Ph_V_Hz)##other##,Power Supply Cable (No x mm2)##other##,Power Supply Cable (No x AWG)##other##,Power and Communication Cable (No x mm2)##other##,Power and Communication Cable (No x AWG)##other##,Running Current_Rated_Cooling (A)##other##,Running Current_Rated_Heating (A)##other##,Air Flow Rate_Max (CMM)##other##,Air Flow Rate_Max (CFM)##other##,Capacity_Rated_Cooling (kW)##other##,Capacity_Rated_Cooling (Btu/h)##other##,Capacity_Rated_Heating (kW)##other##,Capacity_Rated_Heating (Btu/h)##other##,Power Input_Rated_Cooling (W)##other##,Power Input_Rated_Heatling (W)##other##,Compressor Type##other##,Exterior Color Code##other##,Fan Type##other##,Fan Motor Type##other##,Fan Motor Output (W)##other##,Max Elevation Difference (m)##other##,Max Elevation Difference (ft)##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Operation Range Temperature_Cooling (C)##other##,Operation Range Temperature_Cooling (F)##other##,Operation Range Temperature_Heating (C)##other##,Operation Range Temperature_Heating (F)##other##,Piping Length_Min / Standard / Max (m)##other##,Piping Length_Min / Standard / Max (ft)##other##,Piping Length_No Charge (m)##other##,Piping Length_No Charge (ft)##other##,Refrigerant Type##other##,Refrigerant_Precharge (g)##other##,Refrigerant_Precharge (oz)##other##,Refrigerant_Additional Charge (g/m)##other##,Refrigerant_Additional Charge (oz/ft)##other##,Sound Pressure Level_Rated_Cooling (dB(A))##other##,Sound Pressure Level_Rated_Heating (dB(A))##other##
"DC24RQ.U24",Single Inverter,DC24RQ.U24,3UM24K21ZA,U24A,870 x 650 x 330,-,15.88,5/8,6.35,1/4,25,1_220-240_50,3 x 2.5,-,4 x 1,-,9.80,10.00,49.0,-,6.60,22520,7.50,25591,2164,2238,Twin Rotary,Munsell 9.54Y 8.34/1.31 (RAL 9001),Propeller Fan,BLDC,85,15,49.2,46,101.4,-15 ~ 48 (DB),-,-10 ~ 18 (WB),-,3 / 7.5 / 30,9.8 / 24.6 / 98.4,7.5,24.6,R32,1100,38.8,20,0.22,54,57
"PC24SQ.U24",Single Inverter,PC24SQ.U24,S3UM24K22FA,U24A,870 x 650 x 330,-,15.88,5/8,6.35,1/4,25,1_220-240_50,3 x 2.5,-,4 x 1,-,9.80,10.00,49.0,-,6.60,22520,7.50,25591,2164,2238,Twin Rotary,Munsell 9.54Y 8.34/1.31 (RAL 9001),Propeller Fan,BLDC,85,15,49.2,46,101.4,-15 ~ 48 (DB),-,-10 ~ 18 (WB),-,3 / 7.5 / 30,9.8 / 24.6 / 98.4,7.5,24.6,R32,1100,38.8,20,0.22,54,57
"S24EQ.U24",Single Inverter,S24EQ.U24,S3UNW24K23BA,U24A,870 x 650 x 330,-,15.88,5/8,6.35,1/4,25,1_220-240_50,3 x 2.5,-,4 x 1,-,9.80,10.00,49.0,-,6.60,22520,7.50,25591,2164,2238,Twin Rotary,Munsell 9.54Y 8.34/1.31 (RAL 9001),Propeller Fan,BLDC,85,15,49.2,46,101.4,-15 ~ 48 (DB),-,-10 ~ 18 (WB),-,3 / 7.5 / 30,9.8 / 24.6 / 98.4,7.5,24.6,R32,1100,38.8,20,0.22,54,57
"AC24BQ.U24",Single Inverter,AC24BQ.U24,S3UM24K2RZA,U24A,870 x 650 x 330,-,15.88,5/8,6.35,1/4,25,1_220-240_50,3 x 2.5,-,4 x 1,-,9.80,10.00,49.0,-,6.60,22520,7.50,25591,2164,2238,Twin Rotary,Munsell 9.54Y 8.34/1.31 (RAL 9001),Propeller Fan,BLDC,85,15,49.2,46.4,102.3,-15 ~ 48 (DB),-,-10 ~ 18 (WB),-,3 / 7.5 / 30,9.8 / 24.6 / 98.4,7.5,24.6,R32,1100,38.8,20,0.22,54,57

