,Chassis name##other##,Communication Cable (mm2)##other##,Compressor Type##other##,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Air Flow Rate (CFM)##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (kW)##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,MCA (A)##other##,Model name##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Charge (kg)##other##,Refrigerant Charge (lbs)##other##,Refrigerant Type##other##,Sound Pressure Level Cooling (dB(A))##other##,Sound Pressure Level Heating (dB(A))##other##,Temp Operating Range (Cooling)(C)##other##,Temp Operating Range (Cooling)(F)##other##,Temp Operating Range (Heating)(C)##other##,Temp Operating Range (Heating)(F)##other##,Type##other##,Water Inlet Connection Diameter##pipe_size##Millimeters,Water Outlet Connection Diameter##pipe_size##Millimeters
"ZHBW126A0",UN3,3 x 6.0,Hermetic Motor Compressor,-,12,-,"1,239 x 1,380 x 330",-,60.0 x 2,124 x 2,Propeller,-,12,33,ZHBW126A0 [HM121M U33],124.8,-,4.44,4.29,"1, 220-240, 50",2.4,-,R32,-,-,5 ~ 27,-,15 ~ 65,-,Therma V Monobloc,25,25
"ZHBW146A0",UN3,3 x 6.0,Hermetic Motor Compressor,-,14,-,"1,239 x 1,380 x 330",-,60.0 x 2,124 x 2,Propeller,-,14,34,ZHBW146A0 [HM141M U33],124.8,-,5.38,4.29,"1, 220-240, 50",2.4,-,R32,-,-,5 ~ 27,-,15 ~ 65,-,Therma V Monobloc,25,25
"ZHBW166A0",UN3,3 x 6.0,Hermetic Motor Compressor,-,16,-,"1,239 x 1,380 x 330",-,60.0 x 2,124 x 2,Propeller,-,16,35,ZHBW166A0 [HM161M U33],124.8,-,6.4,4.29,"1, 220-240, 50",2.4,-,R32,-,-,5 ~ 27,-,15 ~ 65,-,Therma V Monobloc,25,25
"ZHBW128A0",UN3,5 x 4.0,Hermetic Motor Compressor,-,12,-,"1,239 x 1,380 x 330",-,60.0 x 2,124 x 2,Propeller,-,12,14,ZHBW128A0 [HM123M U33],124.8,-,4.44,4.29,"3, 380-415, 50",2.4,-,R32,-,-,5 ~ 27,-,15 ~ 65,-,Therma V Monobloc,25,25
"ZHBW148A0",UN3,5 x 4.0,Hermetic Motor Compressor,-,14,-,"1,239 x 1,380 x 330",-,60.0 x 2,124 x 2,Propeller,-,14,14.5,ZHBW148A0 [HM143M U33],124.8,-,5.38,4.29,"3, 380-415, 50",2.4,-,R32,-,-,5 ~ 27,-,15 ~ 65,-,Therma V Monobloc,25,25
"ZHBW168A0",UN3,5 x 4.0,Hermetic Motor Compressor,-,16,-,"1,239 x 1,380 x 330",-,60.0 x 2,124 x 2,Propeller,-,16,15,ZHBW168A0 [HM163M U33],124.8,-,6.4,4.29,"3, 380-415, 50",2.4,-,R32,-,-,5 ~ 27,-,15 ~ 65,-,Therma V Monobloc,25,25

