,Chassis name##other##,Communication Cable (mm2)##other##,Compressor Type##other##,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Air Flow Rate (CFM)##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (kW)##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,MCA (A)##other##,Model name##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Charge (kg)##other##,Refrigerant Charge (lbs)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Sound Pressure Level Cooling (dB(A))##other##,Sound Pressure Level Heating (dB(A))##other##,Temp Operating Range (Cooling)(C)##other##,Temp Operating Range (Cooling)(F)##other##,Temp Operating Range (Heating)(C)##other##,Temp Operating Range (Heating)(F)##other##,Type##other##
"AHUW056A2",U4,3 x 2.5 (H07RN-F),Hermetic Motor,-,5,-,950 x 834 x 330,-,58.0 x 1,124 x 1,Propeller,-,5,15,AHUW056A2 (HU051 U42),64,-,5/8,15.88,3/8,9.52,1.35,1.07,"1, 220-240, 50",1.55,-,15.88,9.52,R410A,54,54,5 ~ 48,-,-20 ~ 30,-,Therma V
"AHUW076A2",U4,3 x 2.5 (H07RN-F),Hermetic Motor,-,6.4,-,950 x 834 x 330,-,58.0 x 1,124 x 1,Propeller,-,7,15,AHUW076A2 (HU071 U42),64,-,5/8,15.88,3/8,9.52,1.77,1.59,"1, 220-240, 50",1.55,-,15.88,9.52,R410A,54,54,5 ~ 48,-,-20 ~ 30,-,Therma V
"AHUW096A2",U4,3 x 2.5 (H07RN-F),Hermetic Motor,-,7,-,950 x 834 x 330,-,58.0 x 1,124 x 1,Propeller,-,9,15,AHUW096A2 (HU091 U42),64,-,5/8,15.88,3/8,9.52,1.93,2.09,"1, 220-240, 50",1.55,-,15.88,9.52,R410A,54,54,5 ~ 48,-,-20 ~ 30,-,Therma V

