,Chassis name##other##,Communication Cable (mm2)##other##,Compressor Type##other##,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Air Flow Rate (CFM)##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (kW)##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,MCA (A)##other##,Model name##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Charge (kg)##other##,Refrigerant Charge (lbs)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Sound Pressure Level Cooling (dB(A))##other##,Sound Pressure Level Heating (dB(A))##other##,Temp Operating Range (Cooling)(C)##other##,Temp Operating Range (Cooling)(F)##other##,Temp Operating Range (Heating)(C)##other##,Temp Operating Range (Heating)(F)##other##,Type##other##
"AHUW056A3",U4,3 x 4.0 (H07RN-F),Hermetic Motor,-,5,-,950 x 834 x 330,-,58 x 1,124 x 1,Propeller,-,5,19,AHUW056A3,59,-,5/8,15.88,3/8,9.52,1.09,1.01,"1, 220-240, 50",1.8,-,15.88,9.52,R410A,-,-,5 ~ 48,-,-20 ~ 35,-,Therma V Split
"AHUW076A3",U4,3 x 4.0 (H07RN-F),Hermetic Motor,-,7,-,950 x 834 x 330,-,58 x 1,124 x 1,Propeller,-,7,19,AHUW076A3,59,-,5/8,15.88,3/8,9.52,1.56,1.47,"1, 220-240, 50",1.8,-,15.88,9.52,R410A,-,-,5 ~ 48,-,-20 ~ 35,-,Therma V Split
"AHUW096A3",U4,3 x 4.0(H07RN-F),Hermetic Motor,-,9,-,950 x 834 x 330,-,58 x 1,124 x 1,Propeller,-,9,19,AHUW096A3,59,-,5/8,15.88,3/8,9.52,2.37,2.05,"1, 220-240, 50",1.8,-,15.88,9.52,R410A,-,-,5 ~ 48,-,-20 ~ 35,-,Therma V Split

