,Chassis name##other##,Communication Cable (mm2)##other##,Compressor Type##other##,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Air Flow Rate (CFM)##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (kW)##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,MCA (A)##other##,Model name##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Charge (kg)##other##,Refrigerant Charge (lbs)##other##,Refrigerant Type##other##,Sound Pressure Level Cooling (dB(A))##other##,Sound Pressure Level Heating (dB(A))##other##,Temp Operating Range (Cooling)(C)##other##,Temp Operating Range (Cooling)(F)##other##,Temp Operating Range (Heating)(C)##other##,Temp Operating Range (Heating)(F)##other##,Type##other##,Water Inlet Connection Diameter##pipe_size##Millimeters,Water Outlet Connection Diameter##pipe_size##Millimeters
"ZHBW056A0",UN4,3 x 4.0,Hermetic Motor Compressor,-,5.5,-,"1,239 x 834 x 330",-,60.0 x 1,124 x 1,Propeller,-,5.5,21,ZHBW056A0 [HM051M U43],90.8,-,1.96,2.04,"1, 220-240, 50",1.4,-,R32,-,-,5 ~ 27,-,15 ~ 65,-,Therma V Monobloc,25,25
"ZHBW076A0",UN4,3 x 4.0,Hermetic Motor Compressor,-,7,-,"1,239 x 834 x 330",-,60.0 x 1,124 x 1,Propeller,-,7,22,ZHBW076A0 [HM071M U43],90.8,-,2.59,2.04,"1, 220-240, 50",1.4,-,R32,-,-,5 ~ 27,-,15 ~ 65,-,Therma V Monobloc,25,25
"ZHBW096A0",UN4,3 x 4.0,Hermetic Motor Compressor,-,9,-,"1,239 x 834 x 330",-,60.0 x 1,124 x 1,Propeller,-,9,23,ZHBW096A0 [HM091M U43],90.8,-,3.46,2.04,"1, 220-240, 50",1.4,-,R32,-,-,5 ~ 27,-,15 ~ 65,-,Therma V Monobloc,25,25
