,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,MCA (A)##other##,MFA (A)##other##,Model name##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Pressure Level (H/M/L)(dB(A))##other##,Type##other##,Water Inlet Connection Diameter (inch)##other##,Water Inlet Connection Diameter (mm)##pipe_size##Millimeters,Water Outlet Connection Diameter (inch)##other##,Water Outlet Connection Diameter (mm)##pipe_size##Millimeters
"AHNW166T0",-,25,-,-,20-15/32 x 42-17/32 x 13,"520 x 1,080 x 330",54600,16,-,-,AHNW166T0,94,207.2,-,-,5/8,15.88,3/8,9.52,-,6.13,"1, 220-240, 50",15.88,9.52,R410A,-,43,Therma V IDU,1,25,1,25

