,Chassis name##other##,Communication Cable (mm2)##other##,Compressor Type##other##,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Fan Air Flow Rate (CFM)##other##,Fan Air Flow Rate (CMM)##other##,Fan Motor Output (kW)##other##,Fan Type##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,MCA (A)##other##,Model name##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power Input (Cooling)(kW)##other##,Power Input (Heating)(kW)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Charge (kg)##other##,Refrigerant Charge (lbs)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Sound Pressure Level Cooling (dB(A))##other##,Sound Pressure Level Heating (dB(A))##other##,Temp Operating Range (Cooling)(C)##other##,Temp Operating Range (Cooling)(F)##other##,Temp Operating Range (Heating)(C)##other##,Temp Operating Range (Heating)(F)##other##,Type##other##
"AHUW126A3",U3,3 x 6.0 (H07RN-F),Hermetic Motor,-,10.4,-,"950 x 1,380 x 330",-,55 x 2,124 x 2,Propeller,-,12,25,AHUW126A3,94,-,5/8,15.88,3/8,9.52,2.6,2.64,"1, 220-240, 50",2.3,-,15.88,9.52,R410A,-,-,5 ~ 48,-,-20 ~ 35,-,Therma V Split
"AHUW146A3",U3,3 x 6.0 (H07RN-F),Hermetic Motor,-,12,-,"950 x 1,380 x 330",-,55 x 2,124 x 2,Propeller,-,14,25,AHUW146A3,94,-,5/8,15.88,3/8,9.52,3.08,3.18,"1, 220-240, 50",2.3,-,15.88,9.52,R410A,-,-,5 ~ 48,-,-20 ~ 35,-,Therma V Split
"AHUW166A3",U3,3 x 6.0 (H07RN-F),Hermetic Motor,-,13,-,"950 x 1,380 x 330",-,55 x 2,124 x 2,Propeller,-,16,25,AHUW166A3,94,-,5/8,15.88,3/8,9.52,3.6,3.76,"1, 220-240, 50",2.3,-,15.88,9.52,R410A,-,-,5 ~ 48,-,-20 ~ 35,-,Therma V Split
"AHUW128A3",U3,5 x 2.5 (H07RN-F),Hermetic Motor,-,10.4,-,"950 x 1,380 x 330",-,55 x 2,124 x 2,Propeller,-,12,16.1,AHUW128A3,94,-,5/8,15.88,3/8,9.52,2.6,2.64,"1, 380-415, 50",2.3,-,15.88,9.52,R410A,-,-,5 ~ 48,-,-20 ~ 35,-,Therma V Split
"AHUW148A3",U3,5 x 2.5 (H07RN-F),Hermetic Motor,-,12,-,"950 x 1,380 x 330",-,55 x 2,124 x 2,Propeller,-,14,16.1,AHUW148A3,94,-,5/8,15.88,3/8,9.52,3.08,3.18,"1, 380-415, 50",2.3,-,15.88,9.52,R410A,-,-,5 ~ 48,-,-20 ~ 35,-,Therma V Split
"AHUW168A3",U3,5 x 2.5 (H07RN-F),Hermetic Motor,-,13,-,"950 x 1,380 x 330",-,55 x 2,124 x 2,Propeller,-,16,16.1,AHUW168A3,94,-,5/8,15.88,3/8,9.52,3.6,3.76,"3, 380-415, 50",2.3,-,15.88,9.52,R410A,-,-,5 ~ 48,-,-20 ~ 35,-,Therma V Split

