,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,MCA (A)##other##,MFA (A)##other##,Model name##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Pressure Level (H/M/L)(dB(A))##other##,Type##other##,Water Inlet Connection Diameter (inch)##other##,Water Inlet Connection Diameter (mm)##pipe_size##Millimeters,Water Outlet Connection Diameter (inch)##other##,Water Outlet Connection Diameter (mm)##pipe_size##Millimeters
"AHNW16606B0",-,25,-,12,-,"607 x 2,079 x 725",-,16,-,16.1,AHNW16606B0,228,-,-,-,5/8,15.88,3/8,9.52,4,4.18,-,15.88,9.52,R410A,-,27,Therma V IDU(DHW Tank),1,25,1,25

