,Chassis name##other##,Condensate Drain Connection Diameter##pipe_size##Millimeters,Cooling Capacity (Btu/h)##other##,Cooling Capacity (kW)##other##,Dimensions (WxHxD)(inch)##other##,Dimensions (WxHxD)(mm)##other##,Heating Capacity (Btu/h)##other##,Heating Capacity (kW)##other##,MCA (A)##other##,MFA (A)##other##,Model name##other##,Net Weight (kg)##other##,Net Weight (lbs)##other##,Pipe Connection_Drain Side (inch)##other##,Pipe Connection_Drain Side (mm)##other##,Pipe Connection_Gas Side (inch)##other##,Pipe Connection_Gas Side (mm)##other##,Pipe Connection_Liquid Side (inch)##other##,Pipe Connection_Liquid Side (mm)##other##,Power Input (Cooling)(W)##other##,Power Input (Heating)(W)##other##,Power Supply (Ph_V_Hz)##other##,Refrigerant Gas Connection Diameter##pipe_size##Millimeters,Refrigerant Liquid Connection Diameter##pipe_size##Millimeters,Refrigerant Type##other##,Running Current (A)##other##,Sound Pressure Level (H/M/L)(dB(A))##other##,Type##other##,Water Inlet Connection Diameter (inch)##other##,Water Inlet Connection Diameter (mm)##pipe_size##Millimeters,Water Outlet Connection Diameter (inch)##other##,Water Outlet Connection Diameter (mm)##pipe_size##Millimeters
"AHNW03604A2",NK,25,10236,3,19.29 x 33.46 x 12.4,490 x 850 x 315,10236,3,-,21,AHNW03604A2(HN0314 NK2),46,101.4,-,-,1/2,12.7,1/4,6.35,-,-,"1, 220-240, 50",12.7,6.35,R410A,16.7,-,Therma V IDU,1,25,1,25
"AHNW09604A2",NK,25,23885,7,19.29 x 33.46 x 12.4,490 x 850 x 315,30709,9,-,21,AHNW09604A2(HN0914 NK2),48,105.8,-,-,5/8,15.88,3/8,9.52,-,-,"1, 220-240, 50",15.88,9.52,R410A,16.7,-,Therma V IDU,1,25,1,25
"AHNW16606A2",NK,25,45040,13.2,19.29 x 33.46 x 12.4,490 x 850 x 315,54600,16,-,32,AHNW16606A2 (HN1616 NK2),56,123.5,-,-,5/8,15.88,3/8,9.52,-,-,"1, 220-240, 50",15.88,9.52,R410A,25,-,Therma V IDU,1,25,1,25
"AHNW16809A2",NK,25,45040,13.2,19.29 x 33.46 x 12.4,490 x 850 x 315,54600,16,-,-,AHNW16809A2 (HN1639 NK2),51,112.4,-,-,5/8,15.88,3/8,9.52,-,-,"3, 380-415, 50",15.88,9.52,R410A,-,-,Therma V IDU,1,25,1,25

