,Chassis name##other##,Type##other##,Model name (Buyer)##other##,Model name (Factory)##other##,Operation Range (Leaving Water Temperature) Cooling (C DB)##other##,Operation Range (Leaving Water Temperature) Heating (C DB)##other##,Operation Range (Leaving Water Temperature) DHW (C DB)##other##,Water Pump Type##other##,Water Pump Model##other##,Water Pump Motor Type##other##,Water Pump Steps of Pump Performance##other##,Water Pump Power input (W)##other##,Flow Sensor Type##other##,Flow Sensor Model##other##,Flow Sensor Measuring Range (L/min)##other##,Flow Sensor Flow (Trigger point) (L/min)##other##,Water Pressure Sensor Model##other##,Water Pressure Sensor Measuring Range (bar(G))##other##,Expansion Vessel Volume (L)##other##,Expansion Vessel Water pressure (Max) (bar)##other##,Expansion Vessel Water pressure (Pre-charged) (bar)##other##,Relief valve Pressure Limit (bar)##other##,Devices for Water Circuit##other##,Piping Connections Water Circuit Inlet to PHEX (mm(inch))##other##,Piping Connections Water Circuit Inlet to Heat Load (mm(inch))##other##,Piping Connections Water Circuit Outlet from PHEX (mm(inch))##other##,Piping Connections Water Circuit Outlet from Heat Load (mm(inch))##other##,Wiring Connections Power and Communication Cable (mm2xcores)##other##,Sound Power Level Heating (dB(A))##other##,Dimensions Unit WxHxD (mm)##other##,Dimensions Packed Unit WxHxD (mm)##other##,Weight Unit (kg)##other##,Weight Packed Unit (kg)##other##,Exterior Color##other##,Exterior RAL Code##other##
FHNW16606C0,K1,Hydro Unit,HN1616HC NK0,FHNW16606C0,5~27,15~75,15~80,-,-,-,-,-,-,-,-,-,-,-,8,3,1,-,-,Male PT 25.4(1),Male PT 25.4(1),Male PT 25.4(1),Male PT 25.4(1),0.75 x 3C,39,490 x 850 x 315,563 x 1082 x 375,30,35,Noble White,RAL 9016
FHNW16809C0,K1,Hydro Unit,HN1639HC NK0,FHNW16809C0,5~27,15~75,15~80,-,-,-,-,-,-,-,-,-,-,-,8,3,1,-,-,Male PT 25.4(1),Male PT 25.4(1),Male PT 25.4(1),Male PT 25.4(1),0.75 x 3C,39,490 x 850 x 315,563 x 1082 x 375,30,35,Noble White,RAL 9016
